**399th Aircraft Sanitization Checklist**

**March 2020**

## Prior to Flight

What to bring with you to the airport **prior to flight**:

* Paper towels or disposable sponge
* Kitchen garbage bag
* Plastic gloves (or wash hands immediately after cleaning plane)
* Water / bleach solution (4 TBSP bleach to 1 quart of water)

## Pre-flight

* Wash hands or use hand sanitizer prior to touching anything related to the aircraft.

If you have touched airport doors, gates, your vehicle, or any other object prior to reaching the aircraft, sanitize hands again

## Post flight

Work from the interior outward from the back to the front:

* Seatbelts and connectors
* Headset jacks
* Yokes
* Glareshield
* Sun visors if touched
* All switches
* All knobs
* Elevator Trim Wheel (full rotation then set for Takeoff)
* Rudder Trim Wheel (182 only – full rotation then re-center)
* ALT AIR
* Fuel shutoff knob (if equipped)
* Cowl Flap handle (182 only)
* Center pedestal
* Fuel selector
* COMM and CAP FM Radio buttons (avoid touching GPS screens)
* Avionics knobs
* Audio Panel buttons
* Armrests
* Parking brake handle
* Door and window handles
* Door frame
* Complete filling out the AIF and sanitize the binder
* Gust lock
* Close door and wipe exterior handles
* Wipe baggage door inside and out
* When finished with aircraft cover, sanitize all buckles
* Cowl plugs
* Pitot cover
* Tie down ropes/straps
* Keys
* Combo box – inside and out
* Combo box numbers, rotate through
* Combo box lid

## Trash Disposal

Properly remove gloves without cross contamination. Place gloves into disposable trash bag along with any other trash from the vehicle. Seal the trash bag and dispose of properly.

## CAP Aircraft Sterilization Video

<https://www.youtube.com/watch?v=NOEs_jip-nU&feature=youtu.be>